B E I P R S T V W

## S

sDevice - Static variable in class tw.com.prolific.driver.pl2303.PL2303Driver
setDTR(boolean) - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Switch PL2303HXD DTR on or off
SetReadTimeout(int) - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Set Read Time Out Constant, the default is 5000ms
setRTS(boolean) - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Switch PL2303HXD RTS on or off
setup(PL2303Driver.BaudRate, PL2303Driver.DataBits, PL2303Driver.StopBits, PL2303Driver.Parity, PL2303Driver.FlowControl) - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Setup basic communication parameters on PL2303HXD chip
SetWriteTimeout(int) - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Set Write Time Out Constant, the default is 100ms

B E I P R S T V W